From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: amazingfate <liujianfeng1994@gmail.com>
Date: Thu, 26 Dec 2024 21:47:15 +0100
Subject: [ARCHEOLOGY] rockchip64-6.13: add hdmi1 support to rock5b

> X-Git-Archeology: - Revision 12bb4ea7dfd695901aba31ae4b5260398c932a17: https://github.com/armbian/build/commit/12bb4ea7dfd695901aba31ae4b5260398c932a17
> X-Git-Archeology:   Date: Thu, 26 Dec 2024 21:47:15 +0100
> X-Git-Archeology:   From: amazingfate <liujianfeng1994@gmail.com>
> X-Git-Archeology:   Subject: rockchip64-6.13: add hdmi1 support to rock5b
> X-Git-Archeology:
---
 arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts | 44 +++++++++-
 1 file changed, 42 insertions(+), 2 deletions(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts b/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts
@@ -49,6 +49,17 @@ hdmi0_con_in: endpoint {
 		};
 	};
 
+	hdmi1-con {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi1_con_in: endpoint {
+				remote-endpoint = <&hdmi1_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 		pinctrl-names = "default";
@@ -220,10 +231,32 @@ hdmi0_out_con: endpoint {
 	};
 };
 
+&hdmi1 {
+	pinctrl-0 = <&hdmim0_tx1_cec &hdmim0_tx1_hpd
+		     &hdmim1_tx1_scl &hdmim1_tx1_sda>;
+	status = "okay";
+};
+
+&hdmi1_in {
+	hdmi1_in_vp1: endpoint {
+		remote-endpoint = <&vp1_out_hdmi1>;
+	};
+};
+
+&hdmi1_out {
+	hdmi1_out_con: endpoint {
+		remote-endpoint = <&hdmi1_con_in>;
+	};
+};
+
 &hdptxphy0 {
 	status = "okay";
 };
 
+&hdptxphy1 {
+	status = "okay";
+};
+
 &i2c0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c0m2_xfer>;
@@ -896,11 +929,11 @@ &usb_host2_xhci {
 	status = "okay";
 };
 
-&vop_mmu {
+&vop {
 	status = "okay";
 };
 
-&vop {
+&vop_mmu {
 	status = "okay";
 };
 
@@ -910,3 +943,10 @@ vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
 		remote-endpoint = <&hdmi0_in_vp0>;
 	};
 };
+
+&vp1 {
+	vp1_out_hdmi1: endpoint@ROCKCHIP_VOP2_EP_HDMI1 {
+		reg = <ROCKCHIP_VOP2_EP_HDMI1>;
+		remote-endpoint = <&hdmi1_in_vp1>;
+	};
+};
-- 
Armbian

