From 429717d518e8ab162336302782b040755e6f3d9f Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Mon, 30 Nov 2020 06:14:07 +0100
Subject: arm64: dts: sun50i-a64-pinephone: Bump I2C frequency to 400kHz

High speed. :)

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index 76e55a0e415a..c2746a21b021 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -478,6 +478,7 @@ ov5640_ep: endpoint {
 
 &i2c0 {
 	status = "okay";
+	clock-frequency = <400000>;
 
 	touchscreen@5d {
 		compatible = "goodix,gt917s";
@@ -495,6 +496,7 @@ touchscreen@5d {
 
 &i2c1 {
 	status = "okay";
+	clock-frequency = <400000>;
 
 	/* Alternative magnetometer */
 	af8133j: magnetometer@1c {
-- 
2.35.3

