From 6f11d654b5650b8563abeab166342c07899d4f39 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 13 May 2018 21:00:43 +0200
Subject: ARM: dts: sun8i-h3-orange-pi-pc: Increase max CPUX voltage to 1.4V

When using thermal regulation we can afford to go higher. Also add
regulator-ramp-delay, because regulator takes some time to change
voltage.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-pc.dts | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-pc.dts b/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-pc.dts
index b96e015f54ee..92a58e362004 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-pc.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-pc.dts
@@ -194,7 +194,8 @@ reg_vdd_cpux: regulator@65 {
 		 * Use 1.0V as the minimum voltage instead.
 		 */
 		regulator-min-microvolt = <1000000>;
-		regulator-max-microvolt = <1300000>;
+		regulator-max-microvolt = <1400000>;
+		regulator-ramp-delay = <200>;
 		regulator-boot-on;
 		regulator-always-on;
 	};
-- 
2.35.3

