From 3071728a895acee0ad98869a26eac2d25376718d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Tue, 18 Feb 2020 23:57:20 +0100
Subject: regulator: axp20x: Enable over-temperature protection and 16s reset
 function

Why not? Also why here, but whatever.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/regulator/axp20x-regulator.c | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/drivers/regulator/axp20x-regulator.c b/drivers/regulator/axp20x-regulator.c
index f304d393f5e0..95bb3ffd76b9 100644
--- a/drivers/regulator/axp20x-regulator.c
+++ b/drivers/regulator/axp20x-regulator.c
@@ -92,6 +92,8 @@
 #define AXP22X_WORKMODE_DCDCX_MASK(x)	BIT_MASK(x)
 
 #define AXP22X_MISC_N_VBUSEN_FUNC	BIT(4)
+#define AXP22X_MISC_16S_RESET_FUNC	BIT(3)
+#define AXP22X_MISC_OTP			BIT(2)
 
 #define AXP22X_DCDC1_V_OUT_MASK		GENMASK(4, 0)
 #define AXP22X_DCDC2_V_OUT_MASK		GENMASK(5, 0)
@@ -1778,6 +1780,11 @@ static int axp20x_regulator_probe(struct platform_device *pdev)
 		}
 	}
 
+	// enable 16s power-on reset and over-temperature protection
+	regmap_update_bits(axp20x->regmap, AXP20X_OVER_TMP,
+			   AXP22X_MISC_16S_RESET_FUNC | AXP22X_MISC_OTP,
+			   AXP22X_MISC_16S_RESET_FUNC | AXP22X_MISC_OTP);
+
 	return 0;
 }
 
-- 
2.35.3

