// SPDX-License-Identifier: (GPL-2.0+ OR MIT)

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include "rk3588.dtsi"

/ {
	model = "Mixtile Blade 3";
	compatible = "mixtile,blade3", "rockchip,rk3588";

	aliases {
		mmc0 = &sdhci;
		mmc1 = &sdmmc;
		serial2 = &uart2;
	};

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	vcc12v_dcin: vcc12v-dcin-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc12v_dcin";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
	};

	vcc5v0_sys: vcc5v0-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc5v0_usbdcin: vcc5v0-usbdcin-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_usbdcin";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc5v0_usb: vcc5v0-usb-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_usb";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_usbdcin>;
	};

	pcie20_avdd0v85: pcie20-avdd0v85-regulator {
		compatible = "regulator-fixed";
		regulator-name = "pcie20_avdd0v85";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <850000>;
		regulator-max-microvolt = <850000>;
		vin-supply = <&vdd_0v85_s0>;
	};

	pcie20_avdd1v8: pcie20-avdd1v8-regulator {
		compatible = "regulator-fixed";
		regulator-name = "pcie20_avdd1v8";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&avcc_1v8_s0>;
	};

	pcie30_avdd0v75: pcie30-avdd0v75-regulator {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd0v75";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <750000>;
		regulator-max-microvolt = <750000>;
		vin-supply = <&avdd_0v75_s0>;
	};

	pcie30_avdd1v8: pcie30-avdd1v8-regulator {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd1v8";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&avcc_1v8_s0>;
	};

	vcc3v3_pcie30: vcc3v3-pcie30-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_pcie30";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		enable-active-high;
		regulator-boot-on;
		regulator-always-on;
		gpios = <&gpio1 RK_PB2 GPIO_ACTIVE_HIGH>;
		startup-delay-us = <5000>;
		vin-supply = <&vcc12v_dcin>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie3_vcc3v3_en>;
	};

	vcc_3v3_sd_s0: vcc-3v3-sd-s0-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_3v3_sd_s0";
		gpio = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sdmmc_pwr>;
		enable-active-high;
	};

	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};
};

&combphy0_ps {
	status = "okay";
};

&combphy1_ps {
	status = "okay";
};

&combphy2_psu {
	status = "okay";
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_big0_s0>;
	mem-supply = <&vdd_cpu_big0_mem_s0>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_big0_s0>;
	mem-supply = <&vdd_cpu_big0_mem_s0>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu_big1_s0>;
	mem-supply = <&vdd_cpu_big1_mem_s0>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu_big1_s0>;
	mem-supply = <&vdd_cpu_big1_mem_s0>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;
	status = "okay";

	vdd_cpu_big0_s0: vdd_cpu_big0_mem_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big0_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: vdd_cpu_big1_mem_s0: regulator@43 {
		compatible = "rockchip,rk8603", "rockchip,rk8602";
		reg = <0x43>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big1_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1m2_xfer>;
	status = "okay";

	vdd_npu_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_npu_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <950000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c4 {
	pinctrl-0 = <&i2c4m0_xfer>;
	status = "okay";
};

/* exposed on the 30-pin connector; shows up as i2c-3 */
&i2c5 {
	pinctrl-0 = <&i2c5m3_xfer>;
	status = "okay";
};

&i2s2_2ch {
	pinctrl-names = "default";
	pinctrl-0 = <&i2s2m1_mclk
				 &i2s2m1_lrck
				 &i2s2m1_sclk
				 &i2s2m1_sdi
				 &i2s2m1_sdo>;
	status = "okay";
};

&pcie2x1l0 {
	reset-gpios = <&gpio1 RK_PB4 GPIO_ACTIVE_HIGH>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie2_0_rst>;
	status = "okay";
};

&pcie2x1l1 {
	reset-gpios = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie2_1_rst>;
	status = "okay";
};

&pcie30phy {
	status = "okay";
};

&pcie3x4 {
	reset-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie30>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie3_rst>;
	status = "okay";
};

&pinctrl {
	sdmmc {
		sdmmc_pwr: sdmmc-pwr {
			rockchip,pins = <0 RK_PB7 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pcie2 {
		pcie2_0_rst: pcie2-0-rst {
			rockchip,pins = <1 RK_PB4 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie2_1_rst: pcie2-1-rst {
			rockchip,pins = <4 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pcie3 {
		pcie3_rst: pcie3-rst {
			rockchip,pins = <4 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie3_vcc3v3_en: pcie3-vcc3v3-en {
			rockchip,pins = <1 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
};

&pwm8 {
    pinctrl-names = "active";
	pinctrl-0 = <&pwm8m2_pins>;
	status = "okay";
};

&pwm14 {
	pinctrl-0 = <&pwm14m2_pins>;
	status = "okay";
};

&pwm15 {
	pinctrl-0 = <&pwm15m3_pins>;
	status = "disabled";
};

&spi4 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi4m2_cs0 &spi4m2_pins>;
	num-cs = <1>;
	status = "okay";
};

&saradc {
	status = "okay";
	vref-supply = <&vcc_1v8_s0>;
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	max-frequency = <200000000>;
	// hs400 causes immediate trouble, hs200 works at around 150mb/s
	// mmc-hs400-1_8v;
	// mmc-hs400-enhanced-strobe;
	mmc-hs200-1_8v;
	status = "okay";
};

&sdmmc {
	max-frequency = <150000000>;
	no-sdio;
	no-mmc;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc_3v3_s3>;
	vqmmc-supply = <&vccio_sd_s0>;
	status = "okay";
};

&spi2 {
	status = "okay";
	assigned-clocks = <&cru CLK_SPI2>;
	assigned-clock-rates = <200000000>;
	pinctrl-names = "default";
	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
	num-cs = <1>;

	pmic@0 {
		compatible = "rockchip,rk806";
		spi-max-frequency = <1000000>;
		reg = <0x0>;

		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;

		pinctrl-names = "default";
		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc5v0_sys>;
		vcc6-supply = <&vcc5v0_sys>;
		vcc7-supply = <&vcc5v0_sys>;
		vcc8-supply = <&vcc5v0_sys>;
		vcc9-supply = <&vcc5v0_sys>;
		vcc10-supply = <&vcc5v0_sys>;
		vcc11-supply = <&vcc_2v0_pldo_s3>;
		vcc12-supply = <&vcc5v0_sys>;
		vcc13-supply = <&vcc_1v1_nldo_s3>;
		vcc14-supply = <&vcc_1v1_nldo_s3>;
		vcca-supply = <&vcc5v0_sys>;

		gpio-controller;
		#gpio-cells = <2>;

		rk806_dvs1_null: dvs1-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fun0";
		};

		rk806_dvs2_null: dvs2-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fun0";
		};

		rk806_dvs3_null: dvs3-null-pins {
			pins = "gpio_pwrctrl3";
			function = "pin_fun0";
		};

		regulators {
			vdd_gpu_s0: vdd_gpu_mem_s0: dcdc-reg1 {
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_gpu_s0";
				regulator-enable-ramp-delay = <400>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_lit_s0: vdd_cpu_lit_mem_s0: dcdc-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_cpu_lit_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_log_s0: dcdc-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <750000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_log_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_vdenc_s0: vdd_vdenc_mem_s0: dcdc-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_vdenc_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_ddr_s0: dcdc-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <900000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			vdd2_ddr_s3: dcdc-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vdd2_ddr_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_2v0_pldo_s3: dcdc-reg7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_2v0_pldo_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <2000000>;
				};
			};

			vcc_3v3_s3: dcdc-reg8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_3v3_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vddq_ddr_s0: dcdc-reg9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vddq_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s3: dcdc-reg10 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avcc_1v8_s0: pldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "avcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s0: pldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avdd_1v2_s0: pldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-name = "avdd_1v2_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3_s0: pldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vcc_3v3_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd_s0: pldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vccio_sd_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			pldo6_s3: pldo-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "pldo6_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_0v75_s3: nldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_ddr_pll_s0: nldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_ddr_pll_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			avdd_0v75_s0: nldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "avdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v85_s0: nldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_0v85_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v75_s0: nldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&tsadc {
	status = "okay";
};

&uart2 {
	pinctrl-0 = <&uart2m0_xfer>;
	status = "okay";
};
