From d742191977aca3b6ba39e760ff7c307728e10eb2 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sat, 1 Feb 2020 23:41:18 +0100
Subject: arm64: dts: sun50i-a64: Set fifo-size for uarts

Boot time optimization.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index 9a43bcc2f489..d53a6f7e086a 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -1012,6 +1012,7 @@ uart0: serial@1c28000 {
 			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART0>;
 			resets = <&ccu RST_BUS_UART0>;
 			status = "disabled";
@@ -1023,6 +1024,7 @@ uart1: serial@1c28400 {
 			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART1>;
 			resets = <&ccu RST_BUS_UART1>;
 			status = "disabled";
@@ -1034,6 +1036,7 @@ uart2: serial@1c28800 {
 			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART2>;
 			resets = <&ccu RST_BUS_UART2>;
 			status = "disabled";
@@ -1045,6 +1048,7 @@ uart3: serial@1c28c00 {
 			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART3>;
 			resets = <&ccu RST_BUS_UART3>;
 			status = "disabled";
@@ -1056,6 +1060,7 @@ uart4: serial@1c29000 {
 			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART4>;
 			resets = <&ccu RST_BUS_UART4>;
 			status = "disabled";
-- 
2.35.3

