From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Martin Ayotte <martinayotte@yahoo.ca>
Date: Sat, 5 Jan 2019 09:50:02 -0500
Subject: slow SPIFlash to avoid errors

See Revision ea20f750bfead37ced7b604a44f8f014e317abad
---
 arch/arm64/boot/dts/rockchip/rk3399-rockpro64.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-rockpro64.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-rockpro64.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-rockpro64.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-rockpro64.dtsi
@@ -852,7 +852,7 @@ &spi1 {
 	flash@0 {
 		compatible = "jedec,spi-nor";
 		reg = <0>;
-		spi-max-frequency = <10000000>;
+		spi-max-frequency = <3000000>;
 	};
 };
 
-- 
Armbian

