From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Paolo Sabatino <paolo.sabatino@gmail.com>
Date: Sun, 21 May 2023 13:14:26 +0200
Subject: rk3399: add sd power pin to pinctrl node

---
 arch/arm64/boot/dts/rockchip/rk3399-base.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
@@ -2657,6 +2657,11 @@ sdio0_int: sdio0-int {
 				rockchip,pins =
 					<0 RK_PA4 1 &pcfg_pull_up>;
 			};
+
+			sdmmc_pwr: sdmmc-pwr {
+				rockchip,pins =
+					<0 RK_PA1 1 &pcfg_pull_up>;
+			};
 		};
 
 		sdmmc {
-- 
Armbian

