From 8064f0b57b15ff957b9b33099662870302e42664 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Sat, 16 Oct 2021 21:33:35 +0200
Subject: [PATCH] sunxi: H616 GPU enable hack

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 arch/arm/mach-sunxi/clock_sun50i_h6.c | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/mach-sunxi/clock_sun50i_h6.c b/arch/arm/mach-sunxi/clock_sun50i_h6.c
index 7926394cf7..f12f962530 100644
--- a/arch/arm/mach-sunxi/clock_sun50i_h6.c
+++ b/arch/arm/mach-sunxi/clock_sun50i_h6.c
@@ -16,6 +16,8 @@ void clock_init_safe(void)
 		/* this seems to enable PLLs on H616 */
 		setbits_le32(&prcm->sys_pwroff_gating, 0x10);
 		setbits_le32(&prcm->res_cal_ctrl, 2);
+		/* enable GPU */
+		writel(0, 0x7010254);
 	}
 
 	clrbits_le32(&prcm->res_cal_ctrl, 1);
-- 
2.34.1

