From 671a2d6f20ba155cfcadf114e6d740936ee7088a Mon Sep 17 00:00:00 2001
From: Samuel Holland <samuel@sholland.org>
Date: Sat, 3 Apr 2021 20:53:26 -0500
Subject: ARM: dts: sun8i: a83t: Add MBUS node

Signed-off-by: Samuel Holland <samuel@sholland.org>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi | 15 +++++++++++++++
 1 file changed, 15 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi b/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
index ef62ced26684..04b33b42b414 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
@@ -1056,6 +1056,21 @@ mdio: mdio {
 			};
 		};
 
+		mbus: dram-controller@1c62000 {
+			compatible = "allwinner,sun8i-a83t-mbus";
+			reg = <0x01c62000 0x1000>,
+			      <0x01c63000 0x1000>;
+			reg-names = "mbus", "dram";
+			clocks = <&ccu CLK_BUS_DRAM>,
+				 <&ccu CLK_DRAM>,
+				 <&ccu CLK_MBUS>;
+			clock-names = "apb", "dram", "mbus";
+			#address-cells = <1>;
+			#size-cells = <1>;
+			dma-ranges = <0x00000000 0x40000000 0xc0000000>;
+			#interconnect-cells = <1>;
+		};
+
 		gic: interrupt-controller@1c81000 {
 			compatible = "arm,gic-400";
 			reg = <0x01c81000 0x1000>,
-- 
2.35.3

