From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Paolo Sabatino <paolo.sabatino@gmail.com>
Date: Sat, 1 May 2021 12:41:14 +0000
Subject: Workaround to make several broadcom bluetooth serdev devices work
 even without proper MAC address

---
 drivers/bluetooth/btbcm.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/bluetooth/btbcm.c b/drivers/bluetooth/btbcm.c
index 111111111111..222222222222 100644
--- a/drivers/bluetooth/btbcm.c
+++ b/drivers/bluetooth/btbcm.c
@@ -135,7 +135,7 @@ int btbcm_check_bdaddr(struct hci_dev *hdev)
 		if (btbcm_set_bdaddr_from_efi(hdev) != 0) {
 			bt_dev_info(hdev, "BCM: Using default device address (%pMR)",
 				    &bda->bdaddr);
-			set_bit(HCI_QUIRK_INVALID_BDADDR, &hdev->quirks);
+			//set_bit(HCI_QUIRK_INVALID_BDADDR, &hdev->quirks);
 		}
 	}
 
-- 
Armbian

