From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Wed, 14 Dec 2022 20:15:41 +0300
Subject: arm64: dts: sun50i-h616-orangepi-zero2: reg_usb1_vbus status ok

---
 arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
@@ -56,6 +56,7 @@ reg_usb1_vbus: regulator-usb1-vbus {
 		vin-supply = <&reg_vcc5v>;
 		enable-active-high;
 		gpio = <&pio 2 16 GPIO_ACTIVE_HIGH>; /* PC16 */
+		status = "okay";
 	};
 };
 
-- 
Armbian

