From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Tue, 1 Feb 2022 19:47:29 +0300
Subject: drv:mtd:nand:raw:nand_ids.c add H27UBG8T2BTR-BC nand

---
 drivers/mtd/nand/raw/nand_ids.c | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/drivers/mtd/nand/raw/nand_ids.c b/drivers/mtd/nand/raw/nand_ids.c
index 111111111111..222222222222 100644
--- a/drivers/mtd/nand/raw/nand_ids.c
+++ b/drivers/mtd/nand/raw/nand_ids.c
@@ -50,6 +50,10 @@ struct nand_flash_dev nand_flash_ids[] = {
 	{"SDTNRGAMA 64G 3.3V 8-bit",
 		{ .id = {0x45, 0xde, 0x94, 0x93, 0x76, 0x50} },
 		  SZ_16K, SZ_8K, SZ_4M, 0, 6, 1280, NAND_ECC_INFO(40, SZ_1K) },
+	{"H27UBG8T2BTR-BC 32G 3.3V 8-bit",
+		{ .id = {0xad, 0xd7, 0x94, 0xda, 0x74, 0xc3} },
+		  SZ_8K, SZ_4K, SZ_2M, NAND_NEED_SCRAMBLING, 6, 640,
+		  NAND_ECC_INFO(40, SZ_1K) },
 	{"H27UCG8T2ATR-BC 64G 3.3V 8-bit",
 		{ .id = {0xad, 0xde, 0x94, 0xda, 0x74, 0xc4} },
 		  SZ_8K, SZ_8K, SZ_2M, NAND_NEED_SCRAMBLING, 6, 640,
-- 
Armbian

