From 797e9a51924977c4a8ed90d9f4c5c2af75c97dda Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Sun, 9 May 2021 11:04:58 +0200
Subject: ARM: dts: sunxi: h3/h5: Add hdmi sound card

H3 and H5 support HDMI audio. Add a sound card node for it.

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi | 15 +++++++++++++++
 1 file changed, 15 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
index 7df60515a903..0f19e7c00c50 100644
--- a/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
@@ -106,6 +106,20 @@ de: display-engine {
 		status = "disabled";
 	};
 
+	sound_hdmi: sound_hdmi {
+		compatible = "allwinner,sun9i-a80-hdmi-audio",
+			     "allwinner,sun8i-h3-hdmi-audio";
+		status = "disabled";
+
+		codec {
+			sound-dai = <&hdmi>;
+		};
+
+		cpu {
+			sound-dai = <&i2s2>;
+		};
+	};
+
 	soc {
 		compatible = "simple-bus";
 		#address-cells = <1>;
@@ -818,6 +832,7 @@ csi: camera@1cb0000 {
 		};
 
 		hdmi: hdmi@1ee0000 {
+			#sound-dai-cells = <0>;
 			compatible = "allwinner,sun8i-h3-dw-hdmi",
 				     "allwinner,sun8i-a83t-dw-hdmi";
 			reg = <0x01ee0000 0x10000>;
-- 
2.35.3

