From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: hehopmajieh <hehopmajieh@debian.bg>
Date: Tue, 14 Apr 2020 10:28:16 +0300
Subject: arm:dts:sun7i-a20-olinuxino-micro-emmc Add vqmmc node

---
 arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-micro-emmc.dts | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-micro-emmc.dts b/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-micro-emmc.dts
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-micro-emmc.dts
+++ b/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-micro-emmc.dts
@@ -55,6 +55,7 @@ mmc2_pwrseq: pwrseq {
 
 &mmc2 {
 	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
 	bus-width = <4>;
 	non-removable;
 	mmc-pwrseq = <&mmc2_pwrseq>;
-- 
Armbian

