From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jianfeng Liu <liujianfeng1994@gmail.com>
Date: Thu, 6 Jun 2024 23:29:39 +0800
Subject: arm64: dts: rockchip: Add ap6275p wireless support to ArmSoM Sige7

---
 arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts | 16 ++++++++++
 1 file changed, 16 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts b/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
@@ -283,6 +283,22 @@ &pcie2x1l0 {
 &pcie2x1l1 {
 	reset-gpios = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x300000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+		ranges;
+		device_type = "pci";
+		bus-range = <0x30 0x3f>;
+
+		wifi: wifi@0,0 {
+			compatible = "pci14e4,449d";
+			reg = <0x310000 0 0 0 0>;
+			clocks = <&hym8563>;
+			clock-names = "lpo";
+		};
+	};
 };
 
 /* phy0 - left ethernet port */
-- 
Armbian

