From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Sun, 3 Dec 2017 11:43:08 -0800
Subject: arm64:dts: sun50i-a64-sopine-baseboard Add i2s2 mmc1

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts | 14 ++++++++++
 1 file changed, 14 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
@@ -100,6 +100,10 @@ &i2s2 {
 	status = "okay";
 };
 
+&i2s2 {
+	status = "okay";
+};
+
 &mdio {
 	ext_rgmii_phy: ethernet-phy@1 {
 		compatible = "ethernet-phy-ieee802.3-c22";
@@ -107,6 +111,16 @@ ext_rgmii_phy: ethernet-phy@1 {
 	};
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dldo4>;
+	vqmmc-supply = <&reg_eldo1>;
+	non-removable;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_pins>;
-- 
Armbian

