From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Paolo Sabatino <paolo.sabatino@gmail.com>
Date: Mon, 4 Sep 2023 14:55:50 +0200
Subject: increase timeout for usb3 type C phy init

rockchip64: increase timeout for usb3 type C phy init
---
 drivers/phy/rockchip/phy-rockchip-typec.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/phy/rockchip/phy-rockchip-typec.c b/drivers/phy/rockchip/phy-rockchip-typec.c
index 111111111111..222222222222 100644
--- a/drivers/phy/rockchip/phy-rockchip-typec.c
+++ b/drivers/phy/rockchip/phy-rockchip-typec.c
@@ -904,7 +904,7 @@ static int rockchip_usb3_phy_power_on(struct phy *phy)
 			tcphy_cfg_usb3_to_usb2_only(tcphy, false);
 			goto unlock_ret;
 		}
-		usleep_range(10, 20);
+		usleep_range(100, 200);
 	}
 
 	if (tcphy->mode == MODE_DISCONNECT)
-- 
Armbian

