From 9f7f66239ad389f9b77720ef467ba7d2225868b3 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Sun, 9 May 2021 11:52:43 +0200
Subject: ARM: dts: sun8i: r40: bananapi-m2-ultra: Enable HDMI audio

BananaPi M2 Ultra has HDMI output and thus supports HDMI audio. Enable
it.

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 .../boot/dts/allwinner/sun8i-r40-bananapi-m2-ultra.dts    | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-r40-bananapi-m2-ultra.dts b/arch/arm/boot/dts/allwinner/sun8i-r40-bananapi-m2-ultra.dts
index cd2351acc32f..a91213e8d2c1 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-r40-bananapi-m2-ultra.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-r40-bananapi-m2-ultra.dts
@@ -169,6 +169,10 @@ axp22x: pmic@34 {
 
 #include "axp22x.dtsi"
 
+&i2s2 {
+	status = "okay";
+};
+
 &ir0 {
 	status = "okay";
 };
@@ -304,6 +308,10 @@ &reg_eldo3 {
 	regulator-name = "vdd1v2-sata";
 };
 
+&sound_hdmi {
+	status = "okay";
+};
+
 &tcon_tv0 {
 	status = "okay";
 };
-- 
2.35.3

