From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: SuperKali <hello@superkali.me>
Date: Thu, 20 Mar 2025 19:58:19 +0000
Subject: Fixing USB-A 3.0 on NanoPC T6

Signed-off-by: SuperKali <hello@superkali.me>
---
 arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
@@ -1056,6 +1056,7 @@ &u2phy0 {
 };
 
 &u2phy0_otg {
+	phy-supply = <&vbus5v0_usb>;
 	status = "okay";
 };
 
@@ -1121,6 +1122,7 @@ &usb_host0_ohci {
 
 &usb_host0_xhci {
 	dr_mode = "host";
+	extcon = <&u2phy0>;
 	status = "okay";
 	usb-role-switch;
 
-- 
Armbian

