From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: amazingfate <liujianfeng1994@gmail.com>
Date: Wed, 27 Dec 2023 15:03:57 +0800
Subject: arm64: dts: rock-5b: Slow down emmc freq and add tsadc node

---
 arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts b/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-rock-5b.dts
@@ -440,6 +440,7 @@ &sdhci {
 	no-sdio;
 	no-sd;
 	non-removable;
+	max-frequency = <150000000>;
 	mmc-hs400-1_8v;
 	mmc-hs400-enhanced-strobe;
 	status = "okay";
@@ -495,6 +496,10 @@ flash@0 {
 	};
 };
 
+&tsadc {
+	status = "okay";
+};
+
 &uart6 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart6m1_xfer &uart6m1_ctsn &uart6m1_rtsn>;
-- 
Armbian

