From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: JohnTheCoolingFan <ivan8215145640@gmail.com>
Date: Thu, 13 Jun 2024 11:50:55 +0000
Subject: ARM64: dts: sun50i-h616: BigTreeTech CB1: Enable EMAC1

Signed-off-by: JohnTheCoolingFan <ivan8215145640@gmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi | 18 ++++++++++
 1 file changed, 18 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi
@@ -149,6 +149,24 @@ &cpu0 {
 	cpu-supply = <&reg_dcdc2>;
 };
 
+&emac1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rmii_pins>;
+	phy-mode = "rmii";
+	phy-handle = <&rmii_phy>;
+	phy-supply = <&reg_dldo1>;
+	allwinner,rx-delay-ps = <3100>;
+	allwinner,tx-delay-ps = <700>;
+	status = "okay";
+};
+
+&mdio1 {
+	rmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	vmmc-supply = <&reg_dldo1>;
 	broken-cd;
-- 
Armbian

