From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jianfeng Liu <liujianfeng1994@gmail.com>
Date: Wed, 3 Aug 2022 22:22:55 +0200
Subject: [ARCHEOLOGY] update rockchip64 edge to 5.19 (#4039)

> X-Git-Archeology: - Revision 8c6641e7b79f0d50acdc306d140e586a4e923cf0: https://github.com/armbian/build/commit/8c6641e7b79f0d50acdc306d140e586a4e923cf0
> X-Git-Archeology:   Date: Wed, 03 Aug 2022 22:22:55 +0200
> X-Git-Archeology:   From: Jianfeng Liu <liujianfeng1994@gmail.com>
> X-Git-Archeology:   Subject: update rockchip64 edge to 5.19 (#4039)
> X-Git-Archeology:
> X-Git-Archeology: - Revision 6765f734cc4a22aeaa9f99a3ad28c8c322de26f6: https://github.com/armbian/build/commit/6765f734cc4a22aeaa9f99a3ad28c8c322de26f6
> X-Git-Archeology:   Date: Tue, 25 Oct 2022 11:26:51 +0200
> X-Git-Archeology:   From: Igor Pecovnik <igorpecovnik@users.noreply.github.com>
> X-Git-Archeology:   Subject: Bump rockchip64 edge to 6.0.y (#4337)
> X-Git-Archeology:
> X-Git-Archeology: - Revision 92f1a22d76b987afa7ba555d5b509adc51d689e7: https://github.com/armbian/build/commit/92f1a22d76b987afa7ba555d5b509adc51d689e7
> X-Git-Archeology:   Date: Fri, 16 Dec 2022 13:38:13 +0100
> X-Git-Archeology:   From: Igor Pecovnik <igorpecovnik@users.noreply.github.com>
> X-Git-Archeology:   Subject: Re-add rockchip64 6.0 patches (#4575)
> X-Git-Archeology:
> X-Git-Archeology: - Revision 34ae84fac5d0b66a1ab2d1e51534b7beb13ef245: https://github.com/armbian/build/commit/34ae84fac5d0b66a1ab2d1e51534b7beb13ef245
> X-Git-Archeology:   Date: Fri, 05 May 2023 14:22:00 +0200
> X-Git-Archeology:   From: amazingfate <liujianfeng1994@gmail.com>
> X-Git-Archeology:   Subject: bump rockchip64 edge to v6.3
> X-Git-Archeology:
---
 arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts b/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
@@ -819,6 +819,7 @@ &usb_host0_ohci {
 
 &usb_host0_xhci {
 	extcon = <&usb2phy0>;
+	dr_mode = "host";
 	status = "okay";
 };
 
-- 
Armbian

