From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Gunjan Gupta <viraniac@gmail.com>
Date: Thu, 28 Dec 2023 15:01:03 +0000
Subject: arm64:dts: sun50i-h618-orangepi-zero3 Enable GPU mali

---
 arch/arm64/boot/dts/allwinner/sun50i-h618-orangepi-zero3.dts | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h618-orangepi-zero3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h618-orangepi-zero3.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h618-orangepi-zero3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h618-orangepi-zero3.dts
@@ -28,6 +28,11 @@ &ext_rgmii_phy {
 	motorcomm,clk-out-frequency-hz = <125000000>;
 };
 
+&gpu {
+	mali-supply = <&reg_dcdc1>;
+	status = "okay";
+};
+
 &mmc0 {
 	/*
 	 * The schematic shows the card detect pin wired up to PF6, via an
-- 
Armbian

