From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: JohnTheCoolingFan <ivan8215145640@gmail.com>
Date: Thu, 13 Jun 2024 11:07:35 +0000
Subject: ARM64: dts: sun50i-h616: BigTreeTech CB1: Enable HDMI

Signed-off-by: JohnTheCoolingFan <ivan8215145640@gmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi | 26 ++++++++++
 1 file changed, 26 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-bigtreetech-cb1.dtsi
@@ -26,6 +26,17 @@ chosen {
 		stdout-path = "serial0:115200n8";
 	};
 
+	connector {
+		compatible = "hdmi-connector";
+		type = "d";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -262,6 +273,21 @@ reg_dldo1: dldo1 {
 	};
 };
 
+&de {
+	status = "okay";
+};
+
+&hdmi {
+	hvcc-supply = <&reg_aldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 &cpu0 {
 	cpu-supply = <&reg_dcdc2>;
 	status = "okay";
-- 
Armbian

