From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: hehopmajieh <hehopmajieh@debian.bg>
Date: Tue, 16 Jun 2020 15:40:59 +0300
Subject: arm:dts:sun7i-a20-olinuxino-lime2 enable ldo3 always-on

---
 arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-lime2.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-lime2.dts b/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-lime2.dts
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-lime2.dts
+++ b/arch/arm/boot/dts/allwinner/sun7i-a20-olinuxino-lime2.dts
@@ -237,10 +237,10 @@ &reg_ldo2 {
 };
 
 &reg_ldo3 {
+	regulator-always-on;
 	regulator-min-microvolt = <2800000>;
 	regulator-max-microvolt = <2800000>;
 	regulator-name = "vddio-csi0";
-	regulator-soft-start;
 	regulator-ramp-delay = <1600>;
 };
 
-- 
Armbian

