From 85906a7fbd369ed9a0f6637d1f25eb5ce71d7a4b Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Fri, 28 Jan 2022 15:52:48 +0300
Subject: arm64:dts: sun50i-a64 force mmc0 bus-width

---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index c4272550580c..b216cd417b15 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -568,6 +568,7 @@ mmc0: mmc@1c0f000 {
 			interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
 			max-frequency = <150000000>;
 			status = "disabled";
+			bus-width = <0x4>;
 			#address-cells = <1>;
 			#size-cells = <0>;
 		};
-- 
2.35.3

