From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Tue, 1 Feb 2022 19:43:08 +0300
Subject: arm:dts:sunxi-h3-h5.dtsi add i2s0 i2s1 pins

---
 arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
@@ -463,6 +463,16 @@ i2c2_pins: i2c2-pins {
 				function = "i2c2";
 			};
 
+			i2s0_pins: i2s0-pins {
+				pins = "PA18", "PA19", "PA20", "PA21";
+				function = "i2s0";
+			};
+
+			i2s1_pins: i2s1-pins {
+				pins = "PG10", "PG11", "PG12", "PG13";
+				function = "i2s1";
+			};
+
 			mmc0_pins: mmc0-pins {
 				pins = "PF0", "PF1", "PF2", "PF3",
 				       "PF4", "PF5";
-- 
Armbian

